



***Suggested Specification***

***Please select the ElectriTHERM Tank Size/Input kW, Voltage and Minimum Standby Loss in the UNDERLINED areas of this specification:***

**The Electric water heater will be a Bock ElectriTHERM digital heavy duty water heater with the following features:**

* + **A digital readout for temperature settings and status**
	+ **Tank size of: 50 gallons**
	+ **Input of: 13.5 kW**
	+ **Voltage of: 208v**
	+ **Required minimal Stand by Loss of: 0.85%/hr (50 gal)**
	+ **Dual cold inlets for ease of installation**
	+ **Clean out hole for easy access**
	+ **Dual magnesium anode rods for cathodic protection**
	+ **Incoloy heating elements for superior corrosion resistance**

**The electric water heater will meet or exceed ASHRAE 90.1, will be UL/cUL listed to UL 1453 & CAN/CSA-C22.2 No. 110-94 and UL listed to NSF 5.**

**The electric water heater will have a 5 year tank warranty**

**The electric water heater will be made in the USA.**

**ElectrTHERM Product Attributes to Choose from when filling out Suggested Spec:**

